Updated Procedure for Bluetooth PAN on Raspberry Pi Zero 02/03/2020

**Install the latest “Raspbian Buster with desktop” and install it to an sd card.**

On first boot run

sudo apt-get install -y bluez-tools

Download my shell script which creates a Bluetooth agent service and BT PAN configuration

Change the “123456” on the second line to your desired PIN

wget <https://raw.githubusercontent.com/msilin/PiZeroBTPAN/master/bt.sh>

chmod +x bt.sh

sudo ./bt.sh

sudo reboot

The raspberry pi should now be discoverable.